Altium Designer Pick and Place Locations
C:\git\msk-hw-rtm-bringup-adapter\ALTIUM\production-data\Assembly\Pick Place for RTM_bringup_adapter.txt

========================================================================================================================
File Design Information:

Date:       07/05/26
Time:       16:02
Revision:   32b1c8e8ba494e763ce190248f5c5fac1e2f73b7
Variant:    No variations
Units used: mil

Designator Comment            Layer    Footprint                                 Center-X(mil) Center-Y(mil) Rotation Description                                                                                                 
R6         DNP                TopLayer RESC200X125X60L30N                        229.156       166.069       180      "Resistor, 1.5 kOhm, 1%, 0805"                                                                              
R5         DNP                TopLayer RESC200X125X60L30N                        229.156       257.874       180      "Resistor, 1.5 kOhm, 1%, 0805"                                                                              
C3         100n               TopLayer CAPC200X125X140L50N                       1351.181      7.874         90       "MLCC, 0805, X7R, 50V, 100nF, +/-20%"                                                                       
R4         180                TopLayer RESC200X125X60L30N                        941.242       5.906         270      "Resistor, 180 Ohm, 1%, 0805"                                                                               
C6         4.7u               TopLayer CAPC200X125X140L50N                       750.787       187.008       90       "MLCC, 0805, X5R, 50V, 4.7uF, +/-10%"                                                                       
C7         4.7u               TopLayer CAPC200X125X140L50N                       834.314       187.008       90       "MLCC, 0805, X5R, 50V, 4.7uF, +/-10%"                                                                       
U1         RPI-PICO2-W        TopLayer RPI_Pico2W                                803.937       1917.323      270      "It is a microcontroller board based on the Raspberry Pi RP2350 microcontroller chip."                      
TP1        5001               TopLayer KEY_50xx                                  1772.701      2602.305      0        "PCB Test Point black, 100 piece package"                                                                   
TP2        5001               TopLayer KEY_50xx                                  1772.701      2467.070      0        "PCB Test Point black, 100 piece package"                                                                   
TP3        5001               TopLayer KEY_50xx                                  1772.701      2331.835      0        "PCB Test Point black, 100 piece package"                                                                   
J2         22-04-1031         TopLayer MOLEX_22-04-1031                          -632.991      2828.290      0        "Mini-Latch / KK Wire-to-Board Header, Vertical, with Friction Ramp, 3 Circuits, Tin (Sn) Plating, Natural" 
LD3        150141VS73100      TopLayer PCC-PLCC2P285L35X28H19                    -62.638       2452.506      270      "LED, Top, green SMD PLCC2, 20mA, 2V, 570nm"                                                                
LD2        150141VS73100      TopLayer PCC-PLCC2P285L35X28H19                    1725.299      757.932       180      "LED, Top, green SMD PLCC2, 20mA, 2V, 570nm"                                                                
LD1        150141VS73100      TopLayer PCC-PLCC2P285L35X28H19                    1725.299      1929.978      180      "LED, Top, green SMD PLCC2, 20mA, 2V, 570nm"                                                                
REFT3      REF                TopLayer PCC_REF1.5mm                              1770.345      2899.606      90       "Fiducuial / PCB Reference Marking 1.5mm"                                                                   
REFT2      REF                TopLayer PCC_REF1.5mm                              1764.875      -120.924      90       "Fiducuial / PCB Reference Marking 1.5mm"                                                                   
REFT1      REF                TopLayer PCC_REF1.5mm                              -874.409      -120.866      90       "Fiducuial / PCB Reference Marking 1.5mm"                                                                   
U3         LT1963AEQ-3.3#PBF  TopLayer DPAK6P170_1394X457L127X84T769X1054N       511.417       408.135       0        "LDO Regulator Pos 3.3V 1.5A Automotive 6-Pin(5+Tab) DDPAK"                                                 
U2         APV1121S           TopLayer SOP-4,_mini_flat                          1151.575      -10.236       0        "APV Series 2500 Vrms 1 Channel Surface Mount Photovoltaic Mosfet Driver - SOIC-4"                          
SW1        7914J-1-000E       TopLayer Bourns_7914J                              1589.009      2157.028      180      "Switch Tactile N.O. SPST Round Button J-Hook 0.1A 16VAC 16VDC 100000Cycle 2.94N SMD"                       
R3         180                TopLayer RESC200X125X60L30N                        85.433        2511.845      180      "Resistor, 180 Ohm, 1%, 0805"                                                                               
R2         1.5k               TopLayer RESC200X125X60L30N                        1693.167      641.144       0        "Resistor, 1.5 kOhm, 1%, 0805"                                                                              
R1         180                TopLayer RESC200X125X60L30N                        1551.663      1931.299      0        "Resistor, 180 Ohm, 1%, 0805"                                                                               
Q1         SUM90N03-2M2P-E3   TopLayer VISHAY_DPAK3P254_1524X482L254X74T741X1041 1270.866      397.963       0        "SUM90N03-2M2P-E3 N-channel Mosfet Transistor, 90 A, 30 V, 2+TAB-PIN TO-263"                                
P4         TSW-103-07-G-S     TopLayer Header,_2.54mm,_3-pos,_1-row              954.724       553.675       90       "Header, 2.54mm pitch, 3-pos, 1-row, TSW-103-07-G-S, HTSW-103-07-G-S"                                       
P3         1146720000         TopLayer WEIDMULLER_1146720000                     1451.181      1044.094      90       "2pol right angle Male connector with solder connection"                                                    
P2         1146720000         TopLayer WEIDMULLER_1146720000                     1451.181      1644.094      90       "2pol right angle Male connector with solder connection"                                                    
P1         TSW-103-07-G-S     TopLayer Header,_2.54mm,_3-pos,_1-row              807.545       553.675       270      "Header, 2.54mm pitch, 3-pos, 1-row, TSW-103-07-G-S, HTSW-103-07-G-S"                                       
D3         STPS1L30U          TopLayer DIOM535X362X265L117X207N                  1566.657      2531.496      0        "1A LOW DROP POWER SCHOTTKY RECTIFIER"                                                                      
C5         100n               TopLayer CAPC200X125X140L50N                       1401.213      2171.398      90       "MLCC, 0805, X7R, 50V, 100nF, +/-20%"                                                                       
C4         100n               TopLayer CAPC200X125X140L50N                       1398.989      2372.945      90       "MLCC, 0805, X7R, 50V, 100nF, +/-20%"                                                                       
M1         5223986-1          TopLayer TE_5223986                                -594.134      2442.912      0        "AMC Hardware Key, 0deg"                                                                                    
C2         4.7u               TopLayer CAPC200X125X140L50N                       -348.228      2662.875      0        "MLCC, 0805, X5R, 50V, 4.7uF, +/-10%"                                                                       
C1         4.7u               TopLayer CAPC200X125X140L50N                       -664.809      2662.875      0        "MLCC, 0805, X5R, 50V, 4.7uF, +/-10%"                                                                       
C10        T521X107M025ATE060 TopLayer CAPPM730X430X430L130X240N                 518.439       -55.678       0        "Capacitor, Tantalum, SMD, Polymer, Molded, ESR 60mOhm, Non-Combustible, 100uF, 7343, +/-20%, 1.4A 25V@85C" 
C9         4.7u               TopLayer CAPC200X125X140L50N                       323.847       82.756        0        "MLCC, 0805, X5R, 50V, 4.7uF, +/-10%"                                                                       
C8         4.7u               TopLayer CAPC200X125X140L50N                       917.841       187.008       90       "MLCC, 0805, X5R, 50V, 4.7uF, +/-10%"                                                                       
P5         TSW-102-07-G-S     TopLayer SAMTEC_TSW-102-07-G-S                     1570.866      2378.322      180      "Header, 2.54mm pitch, 2-pos, 1-row, TSW-102-07-G-S, HTSW-102-07-G-S"                                       
R36        180                TopLayer RESC200X125X60L30N                        1003.336      187.008       90       "Resistor, 180 Ohm, 1%, 0805"                                                                               
LD5        150141VS73100      TopLayer PCC-PLCC2P285L35X28H19                    820.669       -7.391        90       "LED, Top, green SMD PLCC2, 20mA, 2V, 570nm"                                                                
J10        DNP                TopLayer GENERIC_HEADER_2X10_2_54MM                40.945        1767.519      90       "Pin header 2x10 2.54mm"                                                                                    
J9         DNP                TopLayer GENERIC_HEADER_2X10_2_54MM                -159.448      1767.519      90       "Pin header 2x10 2.54mm"                                                                                    
J8         DNP                TopLayer GENERIC_HEADER_2X10_2_54MM                -359.842      1767.519      90       "Pin header 2x10 2.54mm"                                                                                    
J31        973028             TopLayer ERNI-973028                               -823.229      1738.188      90       "High Speed Differential Connector, 3Pair 10 Wafers for AMC's"                                              
J6         DNP                TopLayer GENERIC_HEADER_2X10_2_54MM                40.945        698.621       90       "Pin header 2x10 2.54mm"                                                                                    
J5         DNP                TopLayer GENERIC_HEADER_2X10_2_54MM                -159.448      698.621       90       "Pin header 2x10 2.54mm"                                                                                    
J4         DNP                TopLayer GENERIC_HEADER_2X10_2_54MM                -359.842      698.621       90       "Pin header 2x10 2.54mm"                                                                                    
J30        973028             TopLayer ERNI-973028                               -823.229      753.936       90       "High Speed Differential Connector, 3Pair 10 Wafers for AMC's"                                              
J1         22-04-1031         TopLayer MOLEX_22-04-1031                          -315.288      2828.290      0        "Mini-Latch / KK Wire-to-Board Header, Vertical, with Friction Ramp, 3 Circuits, Tin (Sn) Plating, Natural" 
